****: Switch the machine on and off****

****Short press for two seconds to turn on and off****

****M key: Function key****

****Screen Saver: Off ·30 seconds ·1 minute ·2 minutes (optional)****

****Automatic shutdown: Off ·3 minutes ·5 minutes ·10 minutes****

****Hz Light source: 50Hz·60Hz****

****Language options :16 language options****

****When the adjustment date: year, month, day |, minutes, seconds****

****Format: YES/NO****

****Default setting: YES/NO****

****V. Version 1.0; Version: H69G - V1.0-20190824****

****In video mode:****

****Resolution: 1080FHD, 720P, VGA****

****Cyclic recording: Turn off /3 minutes /5 minutes /10 minutes. When the flash memory card is full, the first recording data will be deleted and then the recording will be saved.****

****High dynamic range of HDR: On/off (When on, the recording function will be automatically opened if something moves under the camera, without manual operation.)****

****Exposure compensation: 7 speed options****

****Date label: The screen can be selected to show/close - date time****

****In photo mode:****

****Photo delay: Single shot ·2 seconds ·5 seconds ·10 seconds****

****Photo pixel: 1.3M·2M·5M·8M·10M·12M****

****Consecutive beat: 3 consecutive beats****

****Photo quality: Quality, Standard and compression****

****Sharpness: Strong, standard, soft****

****Color: No · black and white · Nostalgia****

****ISO: Automatic ·100·200·400****

****Exposure Compensation: 7 stops to choose from****

****Photo aid: Anti hand shock open/close****

****Date label: On/off****

****Storage space:****

****Watch: Up · Down remove protection****

****D key: Mode key:****

****Switch: Camera mode · Photo Mode · Playback Mode:****

****Scroll up key, scroll down key, OK key (take photo/video, open key)****

****1: Power supply DC port (Micro USB).****

****2: Flash memory card socket (MicroSD), supporting 1-128GB. More than Class10 speed****

****3: light brightness regulator.****

****4: REST key, system restore button. (If the machine cannot be operated, please press the button in the hole with a needle-shaped sharp object to restart the machine)****

****5: Highlight 8 LED lights, continuous service life of up to 100,000 hours.****

